{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":12},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":15,"rows_kept":23,"merged":[[0,0,0,14],[17,0,17,10],[17,11,17,14],[18,0,18,10],[19,0,19,10]]}
["2023年“P”项目灯具采购报价表"]
["序号","设备名称","规格尺寸","灯具规格","灯具电压","色温","防护等级","光效满足","单位","数量","全费用单价限价（元）","供应商所报单价（元）","金额","设计示意","其他要求"]
[1,"庭院灯（4m）","路灯灯杆均采用整板卷压成型热镀锌钢杆、路灯灯杆壁厚不小于2.5mm；总高度4米；漏电空开C6/2P/0.03A/0.1S；带调光控制器。（含基础预埋件及灯具辅助配件、公园专属LOGO焊接粘贴）","45W/LED","220v","3700K","IP65","100lm/W","根",{"$f":"255+31","v":286},1500,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求求;；\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[2,"庭院灯（7m）","路灯灯杆均采用整板卷压成型热镀锌钢杆、路灯灯杆壁厚不小于2.5mm；总高度7米；漏电空开C6/2P/0.03A/0.1S；带调光控制器。（含基础预埋件及灯具辅助配件、公园专属LOGO焊接粘贴）","120W/LED","220v","3700K","IP65","100lm/W","根",18,2200,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[3,"中杆投光灯","路灯灯杆均采用整板卷压成型热镀锌钢杆、路灯灯杆壁厚不小于3mm；总高度8米；漏电空开C10/4P/0.03A/0.1S。（含基础预埋件及灯具辅助配件、公园专属LOGO焊接粘贴）","4×200W/LED","220v","3700K","IP65","100lm/W","根",8,5000,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[4,"高杆投光灯","路灯灯杆均采用整板卷压成型热镀锌钢杆、路灯灯杆壁厚不小于3mm；总高度8米；漏电空开C10/4P/0.03A/0.1S；（含基础预埋件及灯具辅助配件、公园专属LOGO焊接粘贴）","3x200W/LED","220v","3700K","IP65","100lm/W","根",4,4500,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[5,"投光灯及预埋件","含基础预埋件及灯具辅助配件","50W/LED","220V","3700K","IP65",null,"盏",42,300,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[6,"埋地灯及预埋件","铝合金压铸灯体，不锈钢面盖.，太阳能/动力电两用。（含基础预埋件及灯具辅助配件）","9W/LED","24V","3700K","IP67",null,"盏",42,200,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[7,"点光源及预埋件","含基础预埋件及灯具辅助配件","6W/LED","24V",null,"IP65",null,"盏",400,50,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[8,"LED灯条","4W/米（含基础预埋件及灯具辅助配件）","LED","24V",null,"IP65",null,"米",1150,25,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[9,"洗墙灯","12W/米（含基础预埋件及灯具辅助配件）","LED","24V",null,"IP65",null,"米",65,100,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求；\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[10,"护栏灯","8W/盏（含基础预埋件及灯具辅助配件）","LED","220v",null,"IP65",null,"盏",1200,90,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[11,"涵洞（LED灯带灯）","9W/1m，一米10段，光束角：120（含基础预埋件及灯具辅助配件）","LED","DC24V","RGB","IP65",null,"米",4840,35,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[12,"涵洞（星光灯）","光束角：60（含基础预埋件及灯具辅助配件）","50W/LED","AC22OV","7500K","IP65",null,"个",16,220,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求；\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[13,"涵洞（LED投光灯）","光束角：30（含基础预埋件及灯具辅助配件）","15W/LED","AC22OV","3000K","IP65",null,"个",108,160,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[14,"仿石投光灯","灯身材质：环保树脂（含基础预埋件及灯具辅助配件）","12W/LED","AC22OV","3500K","IP65",null,"个",35,400,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
[15,"发光树桩灯","灯身材质：环保树脂（含基础预埋件及灯具辅助配件）","1x9W/LED","AC22OV","3500K","IP65",null,"个",4,450,{"$nulls":3},"1.LED 光源不低于欧普、飞利浦、雷士的品牌品质要求\n2.所有照明设备均属于室外，质保2年，后期照明出现问题均由供应商负责维修更换。"]
["合计（大写：                                            ），能开具税率：            "]
["注：1.要求报价为含税到场价，开具的发票为1%税率或3%税率或13%税率的增值税专用发票。"]
["    2.所有灯具须符合相关行业质量标准，以实际供应数量按实结算。"]
[null,"                                       ",{"$nulls":4},"报价单位（公章）："]
[{"$nulls":6},"法人或委托代理人及电话："]
[{"$nulls":6},"时间：      年    月    日"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}