{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["水电安装工程"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"水电安装工程","index":0,"n_rows":57,"n_cols":11,"rows_kept":57,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,9,2,10],[4,1,4,2],[4,6,4,7],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[16,1,16,2],[16,6,16,7],[17,1,17,2],[17,6,17,7],[18,1,18,2],[18,6,18,7],[19,1,19,2],[19,6,19,7],[20,1,20,2],[20,6,20,7],[21,1,21,2],[21,6,21,7],[22,1,22,2],[22,6,22,7],[23,1,23,2],[23,6,23,7],[24,1,24,2],[24,6,24,7],[25,1,25,2],[25,6,25,7],[26,1,26,2],[26,6,26,7],[27,1,27,2],[27,6,27,7],[28,1,28,2],[28,6,28,7],[29,1,29,2],[29,6,29,7],[30,1,30,2],[30,6,30,7],[31,1,31,2],[31,6,31,7],[32,1,32,2],[32,6,32,7],[33,1,33,2],[33,6,33,7],[34,1,34,2],[34,6,34,7],[35,1,35,2],[35,6,35,7],[36,1,36,2],[36,6,36,7],[37,1,37,2],[37,6,37,7],[38,1,38,2],[38,6,38,7],[39,1,39,2],[39,6,39,7],[40,1,40,2],[40,6,40,7],[41,1,41,2],[41,6,41,7],[42,1,42,2],[42,6,42,7],[43,1,43,2],[43,6,43,7],[44,1,44,2],[44,6,44,7],[45,1,45,2],[45,6,45,7],[46,1,46,2],[46,6,46,7],[47,1,47,2],[47,6,47,7],[48,1,48,2],[48,6,48,7],[49,1,49,2],[49,6,49,7],[50,1,50,2],[50,6,50,7],[51,1,51,2],[51,6,51,7],[52,1,52,2],[52,6,52,7],[53,1,53,2],[53,6,53,7],[54,1,54,2],[54,6,54,7],[55,1,55,2],[55,6,55,7],[56,0,56,8],[56,9,56,10]],"flags":["formulas_cached_only"]}
["2019年“I”项目水电安装工程量清单与报价表","","","","","","","","","",""]
["工程名称：","","2019年“I”项目水电安装工程","","","","",null,"","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","金额（元）"]
["","","","","","","","",null,"全费用单价","合  计"]
[" "," ","","水"," "," "," ",""," ",null,""]
["1","010101007002","","挖填管沟土方","1.土壤类别：综合考虑 \r\n2.管外径：综合考虑\r\n3.挖沟深度：满足设计及规范要求\r\n4.回填要求：满足设计及规范要求\r\n5.其他：满足设计及规范要求","m3","689.123","","9.28"]
["2","031003001863","","DN25拔插式全铜快速取水阀","1.类型：拔插式快速取水阀\r\n2.材质：全铜\r\n3.规格、压力等级：DN25，VB-708塑料阀门箱，DN25闸阀\r\n4.其他：200*200*200C20砼墩子满足设计及规范要求","个","60","","230.87"]
["3","010404001862","","砂包管","1.砂包管规格详见设计图\r\n2.其他：满足设计及规范要求","m3","262.824","","240.56"]
["4","031001006007","","PE管 DN32","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格 PE管 DN32(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","830.133","","14.00"]
["5","031001006007","","PE管 DN40","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格 PE管 DN40(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","386.9","","15.47"]
["6","031001006007","","PE管 DN50","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格 PE管 DN50(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","261","","22.49"]
["7","031001006007","","PE管 DN80","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格PE管 DN80(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","39","","42.73"]
["8","031001006021","","室外排水管 DN100","1.安装部位：室外\r\n2.介质：雨污水\r\n3.材质、规格：U-PVC排水管 DN100\r\n4.连接形式：粘接\r\n5.阻火圈设计要求：PVC-U聚氯乙烯管道阻火圈\r\n6.压力试验及吹、洗设计要求：满足设计要求\r\n7.未尽事宜满足设计及现行技术、质量验收规范要求","m","130","","21.20"]
["9","031001006021","","室外排水管 DN200","1.安装部位：室外\r\n2.介质：雨污水\r\n3.材质、规格：U-PVC排水管 DN200\r\n4.连接形式：粘接\r\n5.阻火圈设计要求：PVC-U聚氯乙烯管道阻火圈\r\n6.压力试验及吹、洗设计要求：满足设计要求\r\n7.未尽事宜满足设计及现行技术、质量验收规范要求","m","50","","49.27"]
["10","031003005460","","阀门井","1.名称、规格：止回阀及阀门井\r\n2.连接形式：详见设计施工图\r\n3.阀门井做法：采用地面操作立式阀门井，按国标05S502进行施工\r\n4.其余做法：满足设计及施工验收规范要求","座","1","","948.91"]
[" "," ","","电"," "," "," ",""," "]
["11","010101007002","","管沟土方","1.土壤类别：综合考虑 \r\n2.管外径：综合考虑\r\n3.挖沟深度：满足设计及规范要求\r\n4.回填要求：满足设计及规范要求\r\n5.其他：满足设计及规范要求","m3","540.75","","9.28"]
["12","040801010001","","总配电箱MA","1.名称：总配电箱MA \r\n2.型号 ：落地式配电箱\r\n3.规格 ：\r\n4.基础形式、材质、规格 ：根据现场实际情况综合包括在内\r\n5.未尽事宜满足设计和规范要求","台","2","","3221.21"]
["13","040805002847","","庭院灯40W节能灯","1.名称：庭院灯 40W  LED 黄光，高度不低于3.5米单杆带透光罩的庭院灯具，配光类型为半截光型(灯具甲供)\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。路灯灯杆均采用厚度不低于4mm的整板卷压成型热镀锌钢杆，灯杆下杆线为  BVV-450/750V-3x2.5，综合考虑长度为4米，灯杆需提供三类防雷措施。\r\n3.垫层、基础:详见设计图","套","68","","312.85"]
["14","030412004868","","景观石亮化灯具","1.名称 景观石亮化灯具(灯具甲供)\r\n2.型号 12w，黄光，LED，不低于IP66\r\n3.规格 \r\n4.安装形式:详见设计图","套","15","","25.17"]
["15","030412001010","","埋地射灯 6w led灯","1.名称 ：埋地射灯(灯具甲供)\r\n2.型号 ：LED灯\r\n3.规格 ：60w\r\n4.未尽事宜满足设计和规范要求","套","4","","39.84"]
["16","030412001874","","建筑立面照射灯","1.名称 照射灯（甲供）\r\n2.型号 \r\n3.规格 \r\n4.类型","套","718","","14.33"]
["17","040805002847","","特色景观灯柱","1.名称：庭院灯 40W  LED 黄光，高度不低于3.5米单杆带透光罩的庭院灯具，配光类型为半截光型(灯具甲供)\r\n2.其他参数：灯具光源腔和电气腔防护等级不低于IP65；灯具效率不低于70%。路灯灯杆均采用厚度不低于4mm的整板卷压成型热镀锌钢杆，灯杆下杆线为  BVV-450/750V-3x2.5，综合考虑长度为4米，灯杆需提供三类防雷措施。\r\n3.垫层、基础:详见设计图\r\n4.满足设计及其他规范要求\r\n","套","21","","312.85"]
["18","030412004871","","洗墙灯","1.名称 洗墙灯(灯具甲供)\r\n2.型号 18w/米，黄光，LED，不低于IP66\r\n3.规格 \r\n4.安装形式","套","20","","25.17"]
["19","040805002847","","停车场照明灯","1.名称 停车场照明灯(灯具甲供)\r\n2.型号 3*100w，黄光，LED，不低于IP65\r\n3.规格 \r\n4.安装形式","套","6","","312.85"]
["20","030408006867","","电力电缆终端头  YJV-3*4.0mm2","1.户内热缩式电缆头\r\n2.四芯\r\n3.1KV以后终端头\r\n4.满足设计及规范要求","个","2","","76.76"]
["21","030408001003","","电力电缆 YJV-3*4.0mm2","1.名称 :电力电缆 \r\n2.型号 :YJV-3*4.0mm2\r\n3.规格 :YJV-3*4.0mm2\r\n4.材质 :铜芯\r\n5.敷设方式、部位 ：穿管敷设\r\n6.未尽事宜满足设计和规范要求","m","2575.926","","15.71"]
["22","030408006867","","电力电缆终端头  YJV-3*2.5mm2","1.户内热缩式电缆头\r\n2.四芯\r\n3.1KV以后终端头\r\n4.满足设计及规范要求","个","2","","76.76"]
["23","030408001003","","电力电缆 YJV-3*2.5mm2","1.名称 :电力电缆 \r\n2.型号 :YJV-3*2.5mm2\r\n3.规格 :YJV-3*2.5mm2\r\n4.材质 :铜芯\r\n5.敷设方式、部位 ：穿管敷设\r\n6.未尽事宜满足设计和规范要求","m","1000","","13.33"]
["24","030411001005","","配管 PVC25","1.名称 :配管 PC25\r\n2.材质 :塑料管\r\n3.规格 ：PC25\r\n4.配置形式 ：埋地暗敷\r\n5.接地要求 ：详设计要求\r\n6.未尽事宜满足设计和规范要求","m","2575","","13.94"]
["25","030411001005","","配管 PVC16","1.名称 :配管 PC16\r\n2.材质 :塑料管\r\n3.规格 ：PC16\r\n4.配置形式 ：埋地暗敷\r\n5.接地要求 ：详设计要求\r\n6.未尽事宜满足设计和规范要求","m","1000","","12.11"]
["26","040803007182","","铺砂、盖保护板（砖）一根管线","1.名称：砖保护层\r\n2.其他：满足设计及规范要求，做法详设计","m","2575","","11.25"]
["27","030411001007","","配管 SC50","1.名称 :配管 SC50\r\n2.材质 :钢管\r\n3.规格 ：SC50\r\n4.配置形式 ：埋地暗敷\r\n5.接地要求 ：详设计要求\r\n6.未尽事宜满足设计和规范要求","m","250","","43.45"]
["28","040205001014","","手孔井","1.材料品种 ：砖砌\r\n2.规格尺寸 ：详设计图纸\r\n3.盖板材质、规格 ：钢筋混凝土井盖\r\n4.基础、垫层：材料品种、厚度：详设计图纸\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","座","31","","274.36"]
[" "," ","","景观照明工程"," "," "," ",""," "]
["1","041001008003","","拆除混凝土路面","1、工作内容：破除混凝土路面，破除的混凝土自行弃置\r\n2.强度等级","m3","25","","68.52"]
["2","010101007002","","挖填管沟土方","1.土壤类别：综合考虑 \r\n2.管外径：综合考虑\r\n3.挖沟深度：满足设计及规范要求\r\n4.回填要求：满足设计及规范要求\r\n5.其他：满足设计及规范要求","m3","650.58","","9.28"]
["3","030411001001","","HDPE高压碳素螺旋管 40管","1.名称：塑料管\r\n2.材质：HDPE高压碳素螺旋管\r\n3.规格：40\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.包括穿引线、支（吊）架、防火堵洞、刨沟槽、凿（压）槽和恢复处理\r\n7.其他：满足设计及规范要求","m","1390","","16.94"]
["4","030411001001","","HDPE高压碳素螺旋管 50管","1.名称：塑料管\r\n2.材质：HDPE高压碳素螺旋管\r\n3.规格：50\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.包括穿引线、支（吊）架、防火堵洞、刨沟槽、凿（压）槽和恢复处理\r\n7.其他：满足设计及规范要求","m","507","","20.32"]
["5","030411001001","","HDPE高压碳素螺旋管 100管","1.名称：塑料管\r\n2.材质：HDPE高压碳素螺旋管\r\n3.规格：100\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.包括穿引线、支（吊）架、防火堵洞、刨沟槽、凿（压）槽和恢复处理\r\n7.其他：满足设计及规范要求","m","1080","","25.19"]
["6","030411001001","","HDPE高压碳素螺旋管 65管","1.名称：塑料管\r\n2.材质：HDPE高压碳素螺旋管\r\n3.规格：65\r\n4.配置形式：综合考虑\r\n5.接地要求：满足设计及规范要求 \r\n6.包括穿引线、支（吊）架、防火堵洞、刨沟槽、凿（压）槽和恢复处理\r\n7.其他：满足设计及规范要求","m","121","","25.43"]
["7","040205001014","","手孔井","1.材料品种 ：砖砌\r\n2.规格尺寸 ：详设计图纸\r\n3.盖板材质、规格 ：钢筋混凝土井盖\r\n4.基础、垫层：材料品种、厚度：详设计图纸\r\n5.未尽事宜满足设计及现行技术、质量验收规范要求","座","36","","274.36"]
[" "," ","","给排水工程"," "," "," ",""," "]
["1","010101007002","","挖填管沟土方","1.土壤类别：综合考虑 \r\n2.管外径：综合考虑\r\n3.挖沟深度：满足设计及规范要求\r\n4.回填要求：满足设计及规范要求\r\n5.其他：满足设计及规范要求","m3","325.332","","9.28"]
["2","031001006001","","HDPE双壁波纹排水塑料管DN300","1.安装部位：室外\r\n2.介质：污水 \r\n3.材质、规格：HDPE双壁波纹排水塑料管DN300 （含胶圈、管件等附件）\r\n4.连接形式：胶圈连接 \r\n5.阻火圈设计要求：详设计 \r\n6.压力试验及吹、洗设计要求：满足设计及规范要求 \r\n7.警示带形式：满足设计及规范要求\r\n8.其他：满足设计及规范要求","m","11","","68.43"]
["3","031001006001","","HDPE双壁波纹排水塑料管DN500","1.安装部位：室外\r\n2.介质：污水 \r\n3.材质、规格：HDPE双壁波纹排水塑料管DN500 （含胶圈、管件等附件）\r\n4.连接形式：胶圈连接 \r\n5.阻火圈设计要求：详设计 \r\n6.压力试验及吹、洗设计要求：满足设计及规范要求 \r\n7.警示带形式：满足设计及规范要求\r\n8.其他：满足设计及规范要求","m","56","","153.67"]
["4","031001006002","","PE室外给水管DN150","1.材质、规格： PE室外给水管DN150\r\n2.连接形式 ：热熔连接\r\n3.阻火圈：满足设计要求 \r\n4.压力试验及吹、洗设计：满足设计要求","m","1072.3","","63.12"]
["5","031001006004","","PE室外给水管DN80","1.材质、规格： PE室外给水管DN80\r\n2.连接形式 ：热熔连接\r\n3.阻火圈：满足设计要求 \r\n4.压力试验及吹、洗设计：满足设计要求","m","10.9","","39.06"]
["6","031001006007","","PE管 DN25","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格 PE管 DN25(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","316","","14.00"]
["7","031001006007","","PE管 DN50","1.安装部位 室外\r\n2.介质 自来水\r\n3.材质、规格 PE管 DN50(含管件)\r\n4.连接形式 热熔\r\n5.阻火圈设计要求 \r\n6.压力试验及吹、洗设计要求 详设计","m","150","","19.13"]
["8","040504001012","","φ1000雨水检查井 ","1.类型：污水检查井\r\n2.直径：Φ1000\r\n3.做法：做法详见02S515图集","座","2","","1509.22"]
["9","010507003010","","300mm宽C20砼排水沟","1.沟截面尺寸：300mm宽；\r\n2.垫层材料种类、厚度：碎石，150mm厚 ；\r\n3.混凝土强度等级：C20 \r\n4.综合单价包含垫层、砼暗沟、盖板等图纸所有工作内容；\r\n","m","360","","138.08"]
["10","010512008864","","盖板:600*300*50厚深灰色荔枝面花岗石","1.单件体积 \r\n2.安装高度 \r\n3.混凝土强度等级 \r\n4.砂浆强度等级、配合比","套","60","","58.25"]
["11","010507003011","","500mm宽C20砼排水沟（现场视情况而定是否还需增加）","1.沟截面尺寸：500mm宽；\r\n2.垫层材料种类、厚度：碎石，150mm厚 ；\r\n3.混凝土强度等级：C20 \r\n4.盖板:500*500*50厚深灰色荔枝面花岗石；\r\n5.综合单价包含垫层、砼暗沟、盖板等图纸所有工作内容；","m","43.76","","174.84"]
["12","031003001863","","DN25拔插式全铜快速取水阀","1.类型：拔插式快速取水阀\r\n2.材质：全铜\r\n3.规格、压力等级：DN25，VB-708塑料阀门箱，DN25闸阀\r\n4.其他：200*200*200C20砼墩子满足设计及规范要求","个","10","","230.87"]
["13","030901012865","","消防栓","1. 安装部位 \r\n2. 型号、规格 \r\n3. 附件材质、规格","套","3","","804.22"]
["合　　计（大写：                                                  ）","","","","","","","","",null,""]